To

Chief Editor, MASU

The following are the technical flaws in the paper.

* SCS-CN method is not applicable to annual rainfall data, it is applicable to only daily rainfall event
* SCS-CN method computes runoff volume (m3)
* Runoff coefficient method computes peak runoff rate (m3/sec) or (m3/day). Hence both cannot be compared.
* Moreover, it is already known that the SCS-CN method is best method for runoff volume estimation

For the above flaws, this paper is **NOT recommended** to publish